*tomakethelunarterrainvehicleltvoperationalfollowthestepsunlockanddislodgethedescentharnesselementsoftheltvsparachutesothatthevehicleisfreetomovechecktheeesystemontheoutercontrolpaneldepressurizethevehiclethevehiclemaynotbefullydepressurizedandwhenyouopenthedoortheleakinggasmaydamageyourspacesuitopenthevehicledoorenterthevehicleandclosethedoorrepressurizethevehiclethiswillallowyoutobreathewithoutyourspacesuitcheckthepropulsionthebatterymanagementunitandthevehiclecontrolsystemlaunchthenavigationsystemandcheckifthepositioningissuccessfulforproperpositioningyoullneedatleastfourlunarsatellitesinsightenterthecoordinateslaunchthevehiclewithsemiautomaticcruisecontrol*